{"text_format":"2","workbook":"xls","n_sheets":4,"sheets":["Übersicht","Blattform","Anlaufmoment","Flächendichte"],"not_rendered":{"charts":4,"images":3,"macros":1,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Übersicht","index":0,"n_rows":31,"n_cols":18,"rows_kept":31,"cut":false,"hidden":false,"merged":[[21,13,23,13],[0,0,0,13],[1,0,1,13],[3,0,11,0],[3,6,10,6]],"flags":["formulas_cached_only"]}
["RoWi-Tool",{"$nulls":16},"Flächenverhältnis"]
["Tool zur Berechnung von Zuschnittschablonen für Rohrwindräder",{"$nulls":16},"akt/opt"]
[]
["Eingaben","Luftdichte","r",1.225,"kg/m³",null,"Ergebnisse","Repellerfläche","A_Rep",0.7853981633974483,"m²",{"$nulls":5},0,1.0034070391122873]
[null,"Schnellaufzahl","l",5,"-",null,null,"optimale Flächendichte",null,7.190402007501994,"%",{"$nulls":5},1,1.0034070391122873]
[null,"Radius Repeller","R_Rep",0.5,"m",null,null,"Anlaufmoment","M_Anl",0.10920981401426376,"Nm"]
[null,"Durchmesser Rohr","D_Rohr",200,"mm",null,null,"Drehzahl bei SLZ","n_SLZ",572.9577951308232,"U/min"]
[null,"Blattanzahl","n_Bl",2,"-",null,null,"Mech. Leistung","P_mech",25.977044254370604,"W"]
[null,"Soll-Anstellwinkel","a_Soll",8,"°",null,null,"Elektr. Leistung","P_elekr",12.988522127185302,"W"]
[null,"Wirk.grad Repeller","h_Rep",25,"%",null,null,"optimale Blattfläche","A_Opt",0.05647328530781392,"m²"]
[null,"Wirk.grad Generator","h_Gen",50,"%",null,null,"aktuelle Blattfläche","A_Akt",0.05666569199965701,"m²"]
[null,"Windgeschwindigkeit","v_W",6,"m/s"]
[{"$nulls":9},"Angleichen der nötigen Rotorfläche über Änderung der Profiltiefe"]
[]
[null,null,null,34,{"$nulls":4},76]
[{"$nulls":12},"Zu hohe Flächendichte"]
[{"$nulls":12},"Blattanzahl verringern"]
[{"$nulls":12},"Rohrdurchmesser erhöhen"]
[{"$nulls":12},"SLZ verringern"]
[]
[]
[{"$nulls":13},"Flächendichte 0% zu groß."]
[{"$nulls":12},"Optimum"]
[]
[]
[]
[]
[{"$nulls":12},"Zu geringe Flächendichte"]
[{"$nulls":12},"Blattanzahl erhöhen"]
[{"$nulls":12},"Rohrdurchmesser verringern"]
[{"$nulls":12},"SLZ erhöhen"]

{"sheet":"Blattform","index":1,"n_rows":27,"n_cols":18,"rows_kept":27,"cut":false,"hidden":false,"merged":[[3,7,3,9],[5,10,8,10],[5,11,8,11]],"flags":["formulas_cached_only"]}
["Blattform und Zuschnitt"]
[]
[]
[null,null,"nötiger Einstellwinkel","Winkel zur Hinterkante","Winkel zur Vorderkante","Gesamtwinkel","Profiltiefe","Profilform (Zuschnitt)",{"$nulls":8},"lam"]
["r/R_Rep","alp_un","eps_eff","eps_0","eps_1","eps","c","Radius [mm]","Hinterkante [mm]","Vorderkante [mm]",{"$nulls":6},2,0.25]
[0,90,82,-7,171,178,310.6686068549907,0,-12.217304763960305,298.4513020910303,"Nicht nutzbarer Bereich","sollte manuell auf geeignete Werte gesetzt werden",{"$nulls":4},3,0.15]
[0.05,75.96375653207353,67.96375653207353,-7,142.92751306414706,149.92751306414706,261.67287422961783,25,-12.217304763960305,249.45556946565756,{"$nulls":6},4,0.08]
[0.1,63.43494882292201,55.43494882292201,-7,117.86989764584402,124.86989764584402,217.9390850548294,50,-12.217304763960305,205.7217802908691,{"$nulls":6},5,0.065]
[0.15,53.13010235415598,45.13010235415598,-7,97.26020470831196,104.26020470831196,181.96838509633378,75,-12.217304763960305,169.75108033237348,{"$nulls":6},6,0.045]
[0.2,45,37,-7,81,88,153.588974175501,100,-12.217304763960305,141.3716694115407,{"$nulls":6},7,0.028]
[0.25,38.659808254090095,30.659808254090095,-7,68.31961650818019,75.31961650818019,131.45752994072188,125,-12.217304763960305,119.24022517676157,{"$nulls":6},8,0.026]
[0.3,33.690067525979785,25.690067525979785,-7,58.38013505195957,65.38013505195957,114.10986220552483,150,-12.217304763960305,101.89255744156453,{"$nulls":6},9,0.021]
[0.35,29.744881296942225,21.744881296942225,-7,50.48976259388445,57.48976259388445,100.33856434531594,175,-12.217304763960305,88.12125958135563]
[0.4,26.56505117707799,18.56505117707799,-7,44.13010235415598,51.13010235415598,89.23886329617257,200,-12.217304763960305,77.02155853221225]
[0.45,23.962488974578182,15.962488974578182,-7,38.924977949156364,45.924977949156364,80.15420741185714,225,-12.217304763960305,67.93690264789686]
[0.5,21.80140948635181,13.801409486351812,-7,34.60281897270362,41.60281897270362,72.61061691848431,250,-12.217304763960305,60.39331215452401]
[0.55,19.98310652189998,11.98310652189998,-7,30.96621304379996,37.96621304379996,66.26354221279274,275,-12.217304763960305,54.04623744883244]
[0.6,18.43494882292201,10.43494882292201,-7,27.86989764584402,34.86989764584402,60.85945237533978,300,-12.217304763960305,48.64214761137947]
[0.65,17.10272896905237,9.102728969052372,-7,25.205457938104743,32.20545793810474,56.20912781324719,325,-12.217304763960305,43.991823049286886]
[0.7,15.945395900922856,7.945395900922856,-7,22.89079180184571,29.89079180184571,52.169273297033605,350,-12.217304763960305,39.951968533073305]
[0.75,14.93141717813755,6.931417178137551,-7,20.8628343562751,27.8628343562751,48.629819845479524,375,-12.217304763960305,36.412515081519224]
[0.8,14.036243467926477,6.036243467926477,-7,19.072486935852954,26.072486935852954,45.50507412138416,400,-12.217304763960305,33.287769357423855]
[0.85,13.240519915187205,5.240519915187205,-7,17.48103983037441,24.48103983037441,42.72747493519076,425,-12.217304763960305,30.51017017123045]
[0.9,12.528807709151511,4.528807709151511,-7,16.057615418303023,23.057615418303023,40.24313067079973,450,-12.217304763960305,28.02582590683943]
[0.95,11.888658039627973,3.8886580396279733,-7,14.777316079255947,21.777316079255947,38.00858678305187,475,-12.217304763960305,25.791282019091565]
[1,11.309932474020213,3.309932474020213,-7,13.619864948040426,20.619864948040426,35.98845346598749,500,-12.217304763960305,23.771148702027187]
[{"$nulls":7},500,null,-12.217304763960305]

{"sheet":"Anlaufmoment","index":2,"n_rows":22,"n_cols":14,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Anlaufmoment",{"$nulls":8},"Auftriebsbeiwert über Formel",null,null,"alpha","Ca"]
[{"$nulls":9},"p_0",0.4593897744996934,null,0,0.4593897744996934]
["Radius [m]","dr [m]","Wirkradius [m]","Wirkfläche [m²]","alpha [°]","ca(alpha)","dF [N]","dM [Nm]",null,"p_1",0.09733228225693928,null,10,1.1033240489065708]
[0.1,{"$nulls":8},"p_2",-0.0037833519927190627,null,20,1.2646839889717116]
[0.125,0.024999999999999994,0.1125,0.0035630813014527855,56.17009587295495,0.6611421892510134,0.05194325935528668,0.005843616677469752,null,"p_3",5.1394631416174564e-05,null,30,1.1637100921479504]
[0.15,0.024999999999999994,0.1375,0.0030695924018280833,61.82506210996506,0.5845368710532606,0.03956409313231459,0.005440062805693257,null,"p_4",-2.4479803067836843e-07,null,40,0.9618913285253132]
[0.175,0.024999999999999994,0.16249999999999998,0.002680605331885509,66.28252558853899,0.5304326407662057,0.03135246645922024,0.005094775799623289,{"$nulls":4},50,0.7619651408310177]
[0.2,0.025000000000000022,0.1875,0.002369717845518608,69.84503376298989,0.486946074542252,0.0254440418983886,0.0047707578559478625,{"$nulls":4},60,0.6079174444294755]
[0.225,0.024999999999999994,0.21250000000000002,0.002117413383850371,72.73622992417191,0.4484666074211594,0.020938441788635905,0.00444941888008513,{"$nulls":4},70,0.48498262732228703]
[0.25,0.024999999999999994,0.2375,0.001909560304129268,75.118050769535,0.4126098971365675,0.01737327174861584,0.004126152040296261,{"$nulls":4},80,0.3196435501482391]
[0.275,0.025000000000000022,0.2625,0.0017359269891409645,77.10774199587411,0.3784655040499043,0.01448659604880645,0.003802731462811693,{"$nulls":4},90,-0.02036845381667618]
[0.3,0.024999999999999967,0.2875,0.0015890374323516542,78.790972327589,0.3457417458983709,0.012114194504308715,0.003482830919988755]
[0.325,0.025000000000000022,0.3125,0.0014633572523573384,80.23116110401281,0.3143797455155166,0.010144099867106205,0.003170031208470689]
[0.35,0.024999999999999967,0.3375,0.0013547300138785083,81.47593756501239,0.28438951833706305,0.008495225905526961,0.0028671387431153496]
[0.375,0.025000000000000022,0.3625,0.0012599886642814153,82.5615934604698,0.25578591609104073,0.007106436172403947,0.002576083112496431]
[0.4,0.025000000000000022,0.3875,0.0011766861745857971,83.51616967696799,0.2285676330722506,0.005930399842155863,0.002298029938835397]
[0.425,0.024999999999999967,0.4125,0.001102906863207185,84.36161830844316,0.2027137245653563,0.0049298145958717645,0.0020335485207971025]
[0.45,0.025000000000000022,0.4375,0.0010371325700748821,85.11533618783064,0.17818646122602644,0.004074905763769932,0.0017827712716493452]
[0.475,0.024999999999999967,0.4625,0.0009781464681731435,85.79126712561026,0.15493582443211018,0.0033416759446318702,0.00154552512439224]
[0.5,0.025000000000000022,0.4875,0.0009249630031129928,86.40070474317591,0.13290381751869518,0.00271063106760888,0.001321432645459329]
[null,null,"Gesamtfläche",0.028332845999828504,null,"Anlaufmoment:",null,0.10920981401426376,"Nm"]
[{"$nulls":5},"Drehzahl bei Ausleg.SLZ",null,572.9577951308232,"U/min"]

{"sheet":"Flächendichte","index":3,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,null,"Sollte nicht verändert werden!"]
["Lambda","Sigma"]
[1.22,75.14]
[1.46,60.16,null,"Flächendichte Polynom"]
[1.78,45.05,null,"p_0",253.82003977159462]
[2.08,35.12,null,"p_1",-253.02283624457525]
[2.32,30.08,null,"p_2",119.89584171481525]
[3.08,18.51,null,"p_3",-32.26654792563684]
[4.03,11.57,null,"p_4",5.1505009943891835]
[4.97,7.21,null,"p_5",-0.4814235806424884]
[6.08,4.63,null,"p_6",0.024300791389719783]
[7.08,3.4,null,"p_7",-0.0005108135188073922]
[8.03,2.59]
[9.03,2.04,null,"Std-Abw.:",0.1663654501252017]
[10.03,1.91]
[11.08,1.77]
[]
[]
[]
[]
[]
["Sigma bei Lambda = ",null,5,7.190402007501994,"%"]