{"text_format":"2","workbook":"xls","n_sheets":4,"sheets":["Übersicht","Blattform","Anlaufmoment","Flächendichte"],"not_rendered":{"charts":4,"images":2,"macros":1,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Übersicht","index":0,"n_rows":31,"n_cols":18,"rows_kept":31,"cut":false,"hidden":false,"merged":[[0,0,0,13],[1,0,1,13],[3,0,11,0],[3,6,10,6],[21,13,23,13]],"flags":["formulas_cached_only"]}
["RoWi-Tool",{"$nulls":16},"Flächenverhältnis"]
["Tool zur Berechnung von Zuschnittschablonen für Rohrwindräder",{"$nulls":16},"akt/opt"]
[]
["Eingaben","Luftdichte","r",1.225,"kg/m³",null,"Ergebnisse","Repellerfläche","A_Rep",2.8352873698647887,"m²",{"$nulls":5},0,0.9981898913623328]
[null,"Schnellaufzahl","l",4,"-",null,null,"optimale Flächendichte",null,11.720475815454485,"%",{"$nulls":5},1,0.9981898913623328]
[null,"Radius Repeller","R_Rep",0.95,"m",null,null,"Anlaufmoment","M_Anl",1.0644493537961237,"Nm"]
[null,"Durchmesser Rohr","D_Rohr",200,"mm",null,null,"Drehzahl bei SLZ","n_SLZ",201.0378228529204,"U/min"]
[null,"Blattanzahl","n_Bl",3,"-",null,null,"Mech. Leistung","P_mech",54.269172313818224,"W"]
[null,"Soll-Anstellwinkel","a_Soll",8,"°",null,null,"Elektr. Leistung","P_elekr",27.134586156909112,"W"]
[null,"Wirk.grad Repeller","h_Rep",25,"%",null,null,"optimale Blattfläche","A_Opt",0.33230917048363806,"m²"]
[null,"Wirk.grad Generator","h_Gen",50,"%",null,null,"aktuelle Blattfläche","A_Akt",0.3317076547837696,"m²"]
[null,"Windgeschwindigkeit","v_W",5,"m/s"]
[{"$nulls":9},"Angleichen der nötigen Rotorfläche über Änderung der Profiltiefe"]
[]
[null,null,null,68,{"$nulls":4},76]
[{"$nulls":12},"Zu hohe Flächendichte"]
[{"$nulls":12},"Blattanzahl verringern"]
[{"$nulls":12},"Rohrdurchmesser erhöhen"]
[{"$nulls":12},"SLZ verringern"]
[]
[]
[{"$nulls":13},"Flächendichte 0% zu klein."]
[{"$nulls":12},"Optimum"]
[]
[]
[]
[]
[{"$nulls":12},"Zu geringe Flächendichte"]
[{"$nulls":12},"Blattanzahl erhöhen"]
[{"$nulls":12},"Rohrdurchmesser verringern"]
[{"$nulls":12},"SLZ erhöhen"]

{"sheet":"Blattform","index":1,"n_rows":27,"n_cols":18,"rows_kept":27,"cut":false,"hidden":false,"merged":[[3,7,3,9],[5,10,8,10],[5,11,8,11]],"flags":["formulas_cached_only"]}
["Blattform und Zuschnitt"]
[]
[]
[null,null,"nötiger Einstellwinkel","Winkel zur Hinterkante","Winkel zur Vorderkante","Gesamtwinkel","Profiltiefe","Profilform (Zuschnitt)",{"$nulls":8},"lam"]
["r/R_Rep","alp_un","eps_eff","eps_0","eps_1","eps","c","Radius [mm]","Hinterkante [mm]","Vorderkante [mm]",{"$nulls":6},2,0.25]
[0,90,82,-24,188,212,370.00980142279786,0,-41.88790204786391,328.12189937493395,"Nicht nutzbarer Bereich","sollte manuell auf geeignete Werte gesetzt werden",{"$nulls":4},3,0.15]
[0.05,78.69006752597979,70.69006752597979,-24,165.38013505195957,189.38013505195957,330.5306894528217,47.50000000000001,-41.88790204786391,288.6427874049578,{"$nulls":6},4,0.08]
[0.1,68.19859051364818,60.198590513648185,-24,144.39718102729637,168.39718102729637,293.90852600032485,95.00000000000001,-41.88790204786391,252.020623952461,{"$nulls":6},5,0.065]
[0.15,59.03624346792648,51.03624346792648,-24,126.07248693585296,150.07248693585296,261.925901368681,142.50000000000003,-41.88790204786391,220.0379993208171,{"$nulls":6},6,0.045]
[0.2,51.34019174590991,43.34019174590991,-24,110.68038349181982,134.68038349181984,235.06161297808737,190.00000000000003,-41.88790204786391,193.17371093022342,{"$nulls":6},7,0.028]
[0.25,45,37,-24,98,122,212.9301687433082,237.50000000000003,-41.88790204786391,171.04226669544428,{"$nulls":6},8,0.026]
[0.3,39.8055710922652,31.805571092265197,-24,87.6111421845304,111.6111421845304,194.79819130315917,285.00000000000006,-41.88790204786391,152.91028925529528,{"$nulls":6},9,0.021]
[0.35,35.53767779197438,27.53767779197438,-24,79.07535558394876,103.07535558394876,179.90043326038284,332.5,-41.88790204786391,138.01253121251892]
[0.4,32.005383208083494,24.005383208083494,-24,72.01076641616699,96.01076641616699,167.570399132531,380.00000000000006,-41.88790204786391,125.68249708466712]
[0.45,29.054604099077146,21.054604099077146,-24,66.10920819815429,90.10920819815429,157.27023694228592,427.50000000000006,-41.88790204786391,115.38233489442203]
[0.5,26.56505117707799,18.56505117707799,-24,61.13010235415598,85.13010235415598,148.58005786397976,475.00000000000006,-41.88790204786391,106.69215581611586]
[0.55,24.443954780416536,16.443954780416536,-24,56.88790956083307,80.88790956083307,141.17603468919376,522.5000000000001,-41.88790204786391,99.28813264132987]
[0.6,22.619864948040426,14.619864948040426,-24,53.23972989608085,77.23972989608086,134.80876000377086,570.0000000000001,-41.88790204786391,92.92085795590694]
[0.65,21.037511025421814,13.037511025421814,-24,50.07502205084363,74.07502205084363,129.28530282746237,617.5,-41.88790204786391,87.39740077959846]
[0.7,19.653824058053306,11.653824058053306,-24,47.30764811610661,71.3076481161066,124.45532414795919,665,-41.88790204786391,82.5674221000953]
[0.75,18.43494882292201,10.43494882292201,-24,44.86989764584402,68.86989764584402,120.20064694314699,712.5,-41.88790204786391,78.31274489528307]
[0.8,17.354024636261325,9.354024636261325,-24,42.70804927252265,66.70804927252266,116.42750973881284,760.0000000000001,-41.88790204786391,74.53960769094893]
[0.85,16.389540334034784,8.389540334034784,-24,40.77908066806957,64.77908066806957,113.06082440728217,807.5,-41.88790204786391,71.17292235941828]
[0.9,15.524110996754256,7.524110996754256,-24,39.04822199350851,63.04822199350851,110.03990613150265,855.0000000000001,-41.88790204786391,68.15200408363874]
[0.95,14.743562836470735,6.743562836470735,-24,37.487125672941474,61.487125672941474,107.31527905803628,902.5,-41.88790204786391,65.42737701017238]
[1,14.036243467926477,6.036243467926477,-24,36.07248693585295,60.07248693585295,104.84626868919135,950.0000000000001,-41.88790204786391,62.95836664132745]
[{"$nulls":7},950.0000000000001,null,-41.88790204786391]

{"sheet":"Anlaufmoment","index":2,"n_rows":22,"n_cols":14,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Anlaufmoment",{"$nulls":8},"Auftriebsbeiwert über Formel",null,null,"alpha","Ca"]
[{"$nulls":9},"p_0",0.4593897744996934,null,0,0.4593897744996934]
["Radius [m]","dr [m]","Wirkradius [m]","Wirkfläche [m²]","alpha [°]","ca(alpha)","dF [N]","dM [Nm]",null,"p_1",0.09733228225693928,null,10,1.1033240489065708]
[0.19000000000000003,{"$nulls":8},"p_2",-0.0037833519927190627,null,20,1.2646839889717116]
[0.23750000000000002,0.04749999999999999,0.21375000000000002,0.010639804815883142,49.82990412704504,0.7650243674446302,0.12463930859414414,0.026641652211998313,null,"p_3",5.1394631416174564e-05,null,30,1.1637100921479504]
[0.28500000000000003,0.047500000000000014,0.26125000000000004,0.009683548551103604,55.5972144538674,0.6696790573452485,0.09929956675235638,0.025942011814053107,null,"p_4",-2.4479803067836843e-07,null,40,0.9618913285253132]
[0.3325,0.04749999999999999,0.30875,0.008899092333384121,60.32837555788021,0.6036304634520642,0.08225512445177034,0.025396269674484096,{"$nulls":4},50,0.7619651408310177]
[0.38000000000000006,0.04750000000000004,0.35625000000000007,0.008252432269331712,64.22846949997106,0.5550523848726998,0.07013939949767396,0.024987161071046354,{"$nulls":4},60,0.6079174444294755]
[0.42750000000000005,0.04749999999999999,0.40375000000000005,0.0077149651067769005,67.47000634641968,0.5161777962232117,0.0609788720784371,0.024620219601668984,{"$nulls":4},70,0.48498262732228703]
[0.47500000000000003,0.04749999999999999,0.45125000000000004,0.007263944501648806,70.19017236192244,0.4825607632596425,0.053674823608304764,0.024220764153247528,{"$nulls":4},80,0.3196435501482391]
[0.5225000000000001,0.04750000000000004,0.49875,0.0068817071981378776,72.49549702125273,0.45184886293240023,0.04761408970409481,0.02374752723991729,{"$nulls":4},90,-0.02036845381667618]
[0.5700000000000001,0.04749999999999999,0.5462500000000001,0.0065546388739579076,74.46809013577152,0.422871896672552,0.04244276751846151,0.023184361756959603]
[0.6175,0.04749999999999999,0.59375,0.006272233992241788,76.17131201326887,0.3950861097188767,0.037945485573382516,0.02253013205919587]
[0.665,0.04749999999999999,0.6412500000000001,0.00602633989066626,77.65433245826245,0.368263025445831,0.033982696832681604,0.021791404343957082]
[0.7125,0.04749999999999999,0.68875,0.00581057931341377,78.95561355951234,0.34232347007871233,0.030458058129073064,0.02097798753639907]
[0.7600000000000001,0.0475000000000001,0.7362500000000001,0.005619918721196557,80.10551327040834,0.31725226607139057,0.02730114547574854,0.020100468356519866]
[0.8075,0.047499999999999876,0.7837500000000001,0.005450347935969742,81.12821751485194,0.29305614465127583,0.024458012407201014,0.019168967224143796]
[0.8550000000000001,0.0475000000000001,0.83125,0.005298642350296151,82.04317433460548,0.26974421965909556,0.02188582161113447,0.01819258921425553]
[0.9025,0.047499999999999876,0.87875,0.0051621856482515355,82.8661630833875,0.24731993269976726,0.019549643421360764,0.017179249156520773]
[0.9500000000000001,0.0475000000000001,0.92625,0.005038836758996667,83.6100968478014,0.2257786221124256,0.017420443563840527,0.01613568585100729]
[null,null,"Gesamtfläche",0.11056921826125654,null,"Anlaufmoment:",null,1.0644493537961237,"Nm"]
[{"$nulls":5},"Drehzahl bei Ausleg.SLZ",null,201.0378228529204,"U/min"]

{"sheet":"Flächendichte","index":3,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,null,"Sollte nicht verändert werden!"]
["Lambda","Sigma"]
[1.22,75.14]
[1.46,60.16,null,"Flächendichte Polynom"]
[1.78,45.05,null,"p_0",253.82003977159462]
[2.08,35.12,null,"p_1",-253.02283624457525]
[2.32,30.08,null,"p_2",119.89584171481525]
[3.08,18.51,null,"p_3",-32.26654792563684]
[4.03,11.57,null,"p_4",5.1505009943891835]
[4.97,7.21,null,"p_5",-0.4814235806424884]
[6.08,4.63,null,"p_6",0.024300791389719783]
[7.08,3.4,null,"p_7",-0.0005108135188073922]
[8.03,2.59]
[9.03,2.04,null,"Std-Abw.:",0.1663654501252017]
[10.03,1.91]
[11.08,1.77]
[]
[]
[]
[]
[]
["Sigma bei Lambda = ",null,4,11.720475815454485,"%"]